{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":171,"n_cols":8,"rows_kept":171,"cut":false,"hidden":false,"merged":[[0,0,3,0],[0,1,3,1],[0,2,0,3],[0,4,0,7],[1,2,2,3],[1,4,1,5],[2,4,2,5],[1,6,2,7],[4,0,10,0],[13,0,16,0],[13,1,16,1],[13,2,13,3],[13,4,13,7],[14,2,15,3],[14,4,14,5],[15,4,15,5],[14,6,15,7],[17,0,45,0],[48,0,51,0],[48,1,51,1],[48,2,48,3],[48,4,48,7],[49,2,50,3],[49,4,49,5],[50,4,50,5],[49,6,50,7],[52,0,70,0],[73,0,76,0],[73,1,76,1],[73,2,73,3],[73,4,73,7],[74,2,75,3],[74,4,74,5],[75,4,75,5],[74,6,75,7],[77,0,84,0],[87,0,90,0],[87,1,90,1],[87,2,87,3],[87,4,87,7],[88,2,89,3],[88,4,88,5],[89,4,89,5],[88,6,89,7],[91,0,92,0],[95,0,98,0],[95,1,98,1],[95,2,95,3],[95,4,95,7],[96,2,97,3],[96,4,96,5],[97,4,97,5],[96,6,97,7],[99,0,115,0],[118,0,121,0],[118,1,121,1],[118,2,118,3],[118,4,118,7],[119,2,120,3],[119,4,119,5],[120,4,120,5],[119,6,120,7],[122,0,125,0],[128,0,131,0],[128,1,131,1],[128,2,128,3],[128,4,128,7],[129,2,130,3],[129,4,129,5],[130,4,130,5],[129,6,130,7],[132,0,139,0],[142,0,145,0],[142,1,145,1],[142,2,142,3],[142,4,142,7],[143,2,144,3],[143,4,143,5],[144,4,144,5],[143,6,144,7],[160,4,160,7],[161,2,162,3],[161,4,161,5],[162,4,162,5],[161,6,162,7],[164,0,170,0],[146,0,157,0],[160,0,163,0],[160,1,163,1],[160,2,160,3]],"flags":["formulas_cached_only"]}
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["Align","DS 410","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"DS 420","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"DS 510","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS 520","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"DS 610","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS 620","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"DS 650","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["Futaba","BLS 153 @6V","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BLS 251","-","-","red","760 µs","blue","560 Hz"]
[null,"BLS 252 @6V","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BLS 253 @6V","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BLS 254","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"BLS 257","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"BLS 351 @6V","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BLS 451 @6V","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[null,"BLS 452 @6V","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BLS 551 @6V","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BLS 651 @6V","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S3115","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"S3116","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"S3151","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S3152","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S3156","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S3156","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S3157","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S9251","-","-","red","760 µs","blue","560 Hz"]
[null,"S9252","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S9253","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"S9254","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"S9255","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S9256","-","-","red","760 µs","blue","560 Hz"]
[null,"S9257","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"S9451","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[null,"S9452","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S9551","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"S9650","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["Graupner/JR","C261","purple","50 Hz","blue","1520 µs","purple","50 Hz"]
[null,"C4041","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"C4421","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"DS285MG/MGHV","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS287MG/MGHV","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS290G","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS3500G","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[null,"DS3517MG","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS368","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS3717HV","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS3781","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS8077","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS8700G","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[null,"DS8717","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS8717HV","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS8900G","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[null,"DS8915","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"DS8917HV","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"MP80","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["HiTec","HS-5065 MG","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"HS-5083 MG","-","-","purple","960 µs","blue flashing","333 Hz"]
[null,"HS-5084 MG","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"HS-5245 MG","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"HS-65 HB/MG","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"HS-6965 HB","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"HS-6975 HB","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"HS-82 MG","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["Logictec","LTS3100","-","-","purple","960 µs","blue flashing","333 Hz"]
[null,"LTS6100","-","-","purple","960 µs","blue flashing","333 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["MKS Servo-tech","BLS-950","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"BLS-970","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"BLS-980","-","-","red","760 µs","blue","560 Hz"]
[null,"BLS-990","-","-","red","760 µs","blue","560 Hz"]
[null,"DS1210","red","120 Hz","blue","1520 µs","purple","50 Hz"]
[null,"DS660A+","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"DS670","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"DS760","-","-","red","760 µs","blue","560 Hz"]
[null,"DS8910/A+","-","-","red","760 µs","blue","560 Hz"]
[null,"DS95","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"DS95-i","-","-","red","760 µs","blue","560 Hz"]
[null,"DS9660/A+","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"DS9670/A+","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"HV300","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"HV380","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"HV767","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"HV787","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["Outrage TORQ","BL 9080 HV","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BL 9088 HV","-","-","red","760 µs","blue","560 Hz"]
[null,"BL 9180 HV","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"BL 9188 HV","-","-","red","760 µs","blue","560 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["robbe","FS 550","purple","50 Hz","blue","1520 µs","purple","50 Hz"]
[null,"FS 550 DIGITAL","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"FS 550 SPEED DIGITAL","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[null,"FS 555 DIGITAL","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"FS 555 SPEED DIGITAL","blue","200 Hz","blue","1520 µs","red","270 Hz"]
[null,"FS 61","purple","50 Hz","blue","1520 µs","purple","50 Hz"]
[null,"FS 61 DIGITAL","blue flashing","165 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"FS 61 SPEED DIGITAL","blue flashing","165 Hz","blue","1520 µs","red flashing","165 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["Savox","SB-2271SG","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"SB-2272MG","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"SC-1251MG","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SC-1257TG","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"SC-1258TG","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SH-0253","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"SH-0254","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"SH-1250MG","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SH-1257MG","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"SH-1290MG","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[null,"SH-1350","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SH-1357","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]
[]
[]
["Manufacturer","Servoname","Swashplate",null,"Tail"]
[null,null,"Frequency",null,"Center-Position",null,"Frequency"]
[{"$nulls":4},"Pulse-Length"]
[null,null,"Color","Hz","Color","µs","Color","Hz"]
["Spektrum","SPMSH3000","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"SPMSH3020","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SPMSH5000","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SPMSH5010","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SPMSH6010","red flashing","65 Hz","blue","1520 µs","purple","50 Hz"]
[null,"SPMSH6040","blue","200 Hz","blue","1520 µs","red flashing","165 Hz"]
[null,"SPMSH6080G","blue","200 Hz","blue","1520 µs","blue flashing","333 Hz"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}